* **AEROCOOL AERO-1000 BLACK GAMING CASE**

Great Water-cooling Support – either 120 or 240mm radiator (Front & Top)

Dual USB 3.0 Super Speed ports and HD audio.

Large Acrylic left side window for clear viewing.

Removable 3.5” HDD cage supports long graphic card up to 410mm.

Supports max. CPU cooler height of 170mm.

Supports max. PSU length of 220mm.

Removable PSU dust filter for easy cleaning.

Shock-proof rubber for 3.5” HDDs and PSU.

Pre-drilled holes for cable management to reduce cable mess.

Supports up to 5×3.5” HDD or 7×2.5” HDD/SSD installation.

Supports max 5 fans – 2x120mm included in the front & 1x120mm included in the rear.

# AEROCOOL AERO-800 GREY GAMING CASE

Superb gaming case aimed for great airflow performance.

Specially designed top metal cover with extended depth to easily install 240mm water cooling system.

Front panel also supports the installation of either 240mm/280mm water cooling system.

Bay covers are designed with a simple flip mechanism for easy removal of bay cover without removing the front panel.

Support hi-end graphic cards up to 390mm.

# AEROCOOL CRUISE STAR ADVANCE BLACK GAMING CASE

ATX / micro ATX / mini-ITX

200 x 483 x 441mm (W x H x D, overall)

2 x USB2.0 + 2 x USB3.0 / HD Audio & Mic + Card Reader – Support SD / microSD(T-Flash) / SDHC / microSDHC upto 32G / SDXC / microSDXC upto 2TB

Support Max. Height of 153 mm For CPU

# AEROCOOL GT-A BLK GAMING CASE

High-End Ultra Mid tower case for gamers and PC enthusiasts.

Solidly constructed chassis interior (0.6mm thickness).

# AEROCOOL GT-R BLACK CASING

High performance case for gamers and DIY enthusiasts.

Supports Long VGA Card up to 293mm.

Install up to 6 fans including large 18cm fan V Superb Airflow.

Includes 1 x USB3.0 internal connectors + 1 x USB2.0 + Audio (HD) & Mic.

Includes 1 x 12cm Black fan (back), 1 x 18cm LED fan (front).

# AEROCOOL VS-92 BLK GAMING CASING

Supports Long VGA Card up to 40cm

Includes Temperature VFD display – shows system temperature

Install up to 10 fans – Superb Airflow

Includes USB3.0 internal connectors x 2 + Audio (HD) + Mic

Includes 1 x 12cm Black fan (back)

# COOLER MASTER ELITE 110 MINI ITX USB 3.0 GAMING CHASSIS

The mini-ITX case with front mesh panel and vents on the top and side panels for better airflow

One 120mm fan in the front (included) and Two 80mm fan on the side (optional)

Dual Super Speed USB 3.0

Supports a 120mm radiator in the front

Supports standard length ATX PSU up to 180mm

Supports graphic card length up to 210mm

Ample storage – up to 3 HDDs / 4 SSDs

# COOLER MASTER ELITE K350 W/ WINDOW CASING

Airflow optimized – mesh on front panel, large vents in the top, rear, bottom, and on the left side panel

Super Speed USB 3.0 port for 10x faster data transfer and 2x faster phone/tablet charging

Comes with a silent 120mm red LED fan in the front; supports up to 4 fans

Large side panel window with fan mounting

Supports high-end graphics cards (GTX 690 & HD 7990)

7 HDD bays (3 tool-free) and 7 expansion slots for great expandability

# COOLER MASTER ELITE RC102 W/ 500W PSU CASING

A budget mini tower with spacious interior to support Mini-ITX, microATX, and ATX

Supports up to 6 fans, including one 120mm fan in the front

Air vents on the side panel for great ventilation

Supports up to 1 ODD, 3 HDDs, and 2 SSDs slot for great expandability

Supports high-end graphics cards up to 322mm / 12.7 inch

Top-mounted PSU installation for easier cable management

Front I/O panel for easy access

# COOLER MASTER K280 W/O POWERSUPPLY CASING

Airflow optimized design – mesh on front panel, vents on side panel, bottom, and rear

Supports up to three 120mm fans

Side panel with fan mounting to cool graphics cards

Super speed USB 3.0 port for 10x faster file transfer and 2x faster phone/tablet charging

Supports high-end graphics cards up to 315mm/12.4”, including NVIDIA GTX 690 and AMD HD 7990

7 HDD bays (2 tool-free) for increased expandability

# COOLER MASTER LAN 241 BLACK CASING

Very compact yet compatible with ATX mainboards and HD 7870 / GTX 570 graphics cards

Integrated side panel lock with unique key

Steel anchor to secure the system to the desk

Subtle yet stylish mirror finish front panel with blue LED stripes and customizable front I/O

Bundled rear exhaust fan and large side panel air vents with optional 120mm fan for excellent airflow

5.25” ODD and 3.5” HDD combo cage at the top with tool-less ODD mounting system

3.5” and 2.5” combo cage at the bottom

# COOLER MASTER MASTER CASE 5 PRO FULL MODULAR BLACK CASING

Clip-And-Click Panel

Dual Chamber Design

Supports 6 x 140mm Fans

Support 3 x Dual-Slot VGA

2 x Slip-And-Clip SSD Pockets

Includes Top Mesh Panel

Includes Top Bracket

# COOLER MASTER STORM TROOPER USB3.0 CASING

Steel body, Front Mesh / Synthetic bezel ATX Full Tower

2 x USB 3.0 / 2 x USB 2.0 / Audio / 1 x eSATA Front Ports

9 External 5.25? Drive Bays

8 converted from 5.25? bay by two 4-in 3 HDD modules