* **APC BX1100LI-MS 1100VA UPS**

#### **BX1100LI-MS Features**

APC Back-UPS 1100VA, 230V, AVR, Universal and IEC Sockets

* Audible alarms

Provides notification of changing utility power and UPS power conditions

* Automatic self-test

Periodic battery self-test ensures early detection of a battery that needs to be replaced.

* Automatic Voltage Regulation (AVR)

Automatically steps up low voltage and steps down high voltage to levels that are suitable for your equipment.

* Battery backup and surge protection

Outlets provide abundant runtime for network gateway equipment and other critical low-power devices, allowing for hours of internet access during a power outage.

* LED Indicators

Provide easy-to-read status of the unit and utility power conditions.

* Resettable circuit breakers

Enables a quick recovery from overload events.

#### **Back-UPS Features & Benefits**

##### **Manageability**

* LED status display

Quickly understand unit and power status with visual indicators.

* Audible alarms

Provides notification of changing utility power and UPS power conditions

##### **Safety**

* Safety-agency approved

Ensures the product has been tested and approved to work safely with the connected service provider equipment and within the specified environment.

##### **Protection**

* Surge only outlets

Protect secondary electronics from surges and spikes without reducing battery power used to run primary electronics during an outage.

* Battery and surge protected outlets

Back up and protect your hardware and data during power outages, surges and spikes.

##### **Availability**

* Automatic self-test

Periodic battery self-test ensures early detection of a battery that needs to be replaced.

* Intelligent battery management

Maximizes battery performance, life, and reliability through intelligent, precision charging.

* Battery failure notification

Provides early-warning fault analysis on batteries enabling timely preventive maintenance

##### **Marketing Features**

* Battery-protected and surge-only outlets

Reserves power capacity and run time for connected equipment that require UPS battery back-up while providing surge only protection for less critical equipment

# APC BX625CI-MS 625VA BLK UPS

APC Back-UPS 625VA, 230V, AVR, Floor, Universal Sockets  
APC Back-UPS,325 Watts /625 VA,Input 230V /Output 230V, Extended runtime model  
Includes: Qty 1 – Detachable 2.0 m NEMA 5-15P to IEC C13 power cord, User Manual  
Standard Lead Time: Usually in Stock  
  
Product Description  
  
**Protection**  
  
Battery and surge protected outlets  
Back up and protect your hardware and data during power outages, surges and spikes.  
Surge only outlets  
Protect secondary electronics from surges and spikes without reducing battery power used to run primary electronics during an outage.  
  
**Availability**  
  
Automatic self-test  
Periodic battery self-test ensures early detection of a battery that needs to be replaced.  
Battery failure notification  
Provides early-warning fault analysis on batteries enabling timely preventive maintenance  
Intelligent battery management  
Maximizes battery performance, life, and reliability through intelligent, precision charging.  
  
**Serviceability**  
  
Resettable circuit breaker  
Easy recovery from overloads; no need to replace a fuse.  
Manageability  
Audible alarms  
Provides notification of changing utility power and UPS power conditions  
LED status display  
Quickly understand unit and power status with visual indicators.  
  
**Safety**  
  
Safety-agency approved  
Ensures the product has been tested and approved to work safely with the connected service provider equipment and within the specified environment.

* **SECURE 220V COMPUTER AVR**

Model: Secure AVR

Automatic Voltage Regulator

Solid state electronic device

220V AVR

500 Watts

Max Capacity: 50VA

Fuse: 5A

Socket: 3 x 220V